This Visual Studio solution can be compiled without modification.
After compiling, before running the executable, make sure:

1. Socket server is on: system -> misc setup -> remote control settings -> socket server on
2. Socket server is 5025: system -> misc setup -> remote control settings -> socket port 5025
3. VNA software is always running when the code is running. The VNA software is the driver for the VNA.


